-std=c99
-DCPU_S32K118
-DTURN_ON_CPU0
-DSTART_FROM_FLASH
-I"D:/myGit/DP1208/16_1-S32K118_BOOTLOADER_BOOT/include"
-I"D:/myGit/DP1208/16_1-S32K118_BOOTLOADER_BOOT/Generated_Code"
-I"D:/myGit/DP1208/16_1-S32K118_BOOTLOADER_BOOT/Sources"
-I"D:/myGit/DP1208/16_1-S32K118_BOOTLOADER_BOOT/SDK/platform/drivers/src/clock/S32K1xx"
-I"D:/myGit/DP1208/16_1-S32K118_BOOTLOADER_BOOT/SDK/platform/devices"
-I"D:/myGit/DP1208/16_1-S32K118_BOOTLOADER_BOOT/SDK/platform/devices/common"
-I"D:/myGit/DP1208/16_1-S32K118_BOOTLOADER_BOOT/SDK/platform/devices/S32K118/include"
-I"D:/myGit/DP1208/16_1-S32K118_BOOTLOADER_BOOT/SDK/platform/devices/S32K118/startup"
-I"D:/myGit/DP1208/16_1-S32K118_BOOTLOADER_BOOT/SDK/platform/drivers/inc"
-I"D:/myGit/DP1208/16_1-S32K118_BOOTLOADER_BOOT/SDK/rtos/osif/"
-I"D:/myGit/DP1208/16_1-S32K118_BOOTLOADER_BOOT/SDK/platform/pal/inc"
-O1
-g
-pedantic
-Wall
-Wextra
-c
-fmessage-length=0
-funsigned-bitfields
-ffunction-sections
-fdata-sections
-fno-common
-Wunused
-mcpu=cortex-m0plus
-mthumb
-mfloat-abi=soft
-specs=nano.specs
-specs=nosys.specs
--sysroot="C:/NXP/S32DS.3.5/S32DS/build_tools/gcc_b1620/gcc-6.3-arm32-eabi/arm-none-eabi/newlib"